;Pixelworks, Inc. Flash loader information file.
;
;(C)2010 Pixelworks, Inc.
;

;-----------------------------------------------------------------------------
; Version information and flash options.
;
; Required parameters are shown below:
; Class             : File class type. Must be "Firmware".
; Chip              : Target system chip identifier (ie. "PWC808").
; SoftwareRevision  : FlashUpgrader software revision supported by this file.
;
; Optional parameters are shown below:
; FlashWrite=Enable : Allow writes to flash ROM area.
; Reset=Enable      : Perform cold start reset in target system after last
;                     file has been downloaded (jump to ffff:0000).
;-----------------------------------------------------------------------------
[Version]
Class=Firmware
Chip=PWC808
SofwareRevision=1.1a

FlashWrite=Enable
Reset=Enable

; THE FOLLOWING PARAMETER IS FOR INTERNAL FACTORY USE ONLY AND SHOULD NOT BE
; RELEASED OUTSIDE OF THE FACTORY. REMOVE IT FROM THIS FILE FOR NON-FACTORY
; USE.
; This option is used to enable flash programming of the Boot ROM block.
; Note: Programming the Boot ROM area can cause the system to become unusable
; and should only be done by experienced personnel.

BootROMWrite=Enable

;-----------------------------------------------------------------------------
; File download information.
;
; Files must be in Intel Extended HEX format. If any portion of this file
; resides in a flash ROM area of the target system, then the entire flash
; sector is erase before writing the new data to the ROM.
;
; Data may be written to RAM or ROM areas, depending on the flash options
; specified in the previous section.
;
; ExecuteFile   : Code file that is invoked immediately after downloading.
;                 Normally used to download the flash loader into RAM and
;                 invoke it so subsiquent files can be downloaded into flash
;                 areas.
;
; File          : Data or code that should only be downloaded, not invoked.
;-----------------------------------------------------------------------------
[DownloadFiles]
File="u-boot.spi-boot"
DDROFFSET=0x0
File="uImage"
DDROFFSET=0x40000
File="root.cramfs"
DDROFFSET=0x200000
File="rootdata.cramfs"
DDROFFSET=0x1300000
File="rw.jffs2"
DDROFFSET=0x1e80000

;NOTE: Enable the following line to automatically erase NVRAM.
;ExecuteFile="EraseNV.hex"
